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Featu Accuracy
model V€902 Vveoo3
DC voltage| 600mV/6V/60V/600V/1000V +(0.5%+3) | +(0.5%¢3)
AC voltage | 600mV/6V/60V/600V/750V +(1%+3) +(1%+3)
BCeument 600UA/6000uA £(1.2%+3) | +(1.2%+3)

60A/600A/1200A £(2%+30) | +(2%+30)
600uA/6000uA H(L5%+3) | (1.5%+3)
AC current | 60A/600A/1000A +(296+30)
60A/600A/1200A +(2%+30)
resistance | 6000/6K0/60k0/600k/6MO H(0.5%+3) | +(0.5%+3)
60MQ E(15%+3) | +(1.5%+3)
9.999nF +(5%+20) | +(5%+20)
capacitance| 99.99nF/999.9nF/9.999uF/99.99uF/999.9F | +(296+5) | £(2%+5)
9.999mF H(5%+5) | +(5%+5)
frequency zz;::;/l 3:.9;:;/:;99%Hx/S‘J.B‘Zka/ £(0.1%+2) | £(0.1%+2)
Duty cycle | 196~999% £(0.1%+2) | £(0.1%+2)
temperature|  (-20~1000) °C  (-4~1832) °F +(2.5%+5) | £(2.5%+5)
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Maximum display 5000 counts
Range mode Auto range or manual range

Diode test v

On-off beep v

Continuity v

Data Hold v

Material ABS

Low battery indication v

Auto power off 15 minutes without operation, auto power off
Backlight v

Update rate 3 times /second

True RMs v

product weight 352g(VC902) 325g(VC903)

Product Size 240mm*90mm*45mm

power supply 1.5V AA baltery*2(VC302) 9V 6F22 battery(VC903)





