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model 71Q8L | z1-Q83 71-QB4
DCvoltage 0.8V-600V | 0.8V-600V | 0.8V-600V
AC voltage 0.8V-600V | 0.8V-600V | 0.8V-600V
AC current 15MA-600A | 15mA-600A | 15mA~600A
resistance 00-40MQ | 00-40MQ | 00-40MQ
capacitance % OnF-4mF | OnF-4mF
diode x v v
Buzzer 0-500 0-500 0-500
frequency 1100kHz | 1-IMHz | 1-IMHz
NCv v v v
temperature x x (30-1000/'C
Zerofire line identification N N v
Surge measurement v v v
Data retention J J M
Automatic shutdown 4 & J
| Screen backlight v v v
flashlight & v v
True RMS v M M
Sampling rate | 3times /sec | 3times/sec | 3times /sec
Display 4000 count | 4000count | 4000 count
Low battery prompt v ] 4





